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💵 Central Bank & Banknote Printing Industry Solution
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Secure. Efficient. Compliant.
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BDS for Central-bank-level: 
Two-Stage Shredding / Dust Extraction & Filtration / Briquetting

Case study • Client A
	Banknote Destruction Machine
	Integrated Baler and Compactor
	Output

	[image: ]
	[image: ]
	[image: ]
	[image: ]

	
	
	[image: ]
	[image: ]






🔒 Industry Background
Banknotes, securities, and confidential financial materials require strict, centralized destruction under national regulations.
In most countries, the Central Bank or Security Printing Corporation mandates that obsolete or damaged banknotes be shredded and compacted before final disposal — ensuring both security and traceability throughout the process. 


💡 YUEDU Solution Overview
Goal: Provide a secure, reliable, and scalable destruction line from in-feed to briquette, with full process traceability and low TCO.
[image: ]
Structure solutions as Standard / Modular / Tailored Lines, all modular & scalable to site constraints and capacities. 
Capacity spans 20–1,000 kg/h (standard) and can be customized up to 1,500 kg/h; shredding, suction, dust filtration and briquetting are delivered as one coherent solution. 
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🧩 Solution Architecture
 ⚙️ System Workflow
Feeding → Shredding → Dust Dust Extraction & Pneumatic Conveying→ Briquetting / Bagging → Monitoring & Control → Storage/Dispatch
[image: Generated image]
Each stage works seamlessly through modular design and centralized PLC control, ensuring continuous operation, data traceability, and high-level security for national banks, mints, and document destruction centers.

🔧 System Composition 
	No.
	Module 模块
	Description (English)

	1️
	Feeding & Preparation Unit
	Handles the intake of obsolete banknotes or securities. Designed with safety covers and anti-jam protection to ensure stable feeding.

	2️
	Shredding Unit
	High-torque industrial shredder reduces banknotes into fine particles of 1–3 mm (up to 1 mm powder for top-security applications).

	3️
	Dust Extraction Unit
	Multi-stage dust collection and filtration system maintains a clean, dust-free working environment and protects operators.

	4️
	Briquetting / Compaction Unit
/ Bagging
	Briquetting / Compaction Unit
Compress shredded particles into Ø90×40 mm briquettes for easy weighing, storage, and traceable disposal.

Bagging / Boxing
More economical and easier to handle and ship for small volumes or polymer notes.

	5️
	PLC & Monitoring with Traceability
	Central control with touch-screen interface integrates all modules, providing real-time operation data, weighing records, and video traceability.
Lockable hoppers and the two-person rule ensure secure batch operations with full auditability.

	6️
	Optional Modules
	Customizable extensions such as conveyor auto-feeding, magnetic separation units, weighing platforms, Remote diagnostics, Reports & dashboards.





Capacity Tiers & Line Types 
	Reference Line 
	Typical Capacity
	Usage Scenarios
	Models

	Standard Line 
	20–300 kg/h
	Security Rooms / Municipal Destruction Room
	Solution C: Cost-Effective 1–3mm Shredding
✔ (6/7) QL300 – QL600 Series – Budget-friendly shredders from $2,000
✔ (7/7) SL500 – SL700 Series – Silent, high-security shredding for offices

	Modular Line 
	300–1,000 kg/h
	Provincial / National Treasury Large-Scale Center
	Solution B: Ultra-Fine 1mm Shredding System
✔ (4/7) 300BM1 – 600BM1 Series – Ultra-fine shredding (1mm) for P-6 compliance 
✔ (5/7) Modular Systems 6002 & 4001 – Customizable with briquetting/baling

	Tailored Line
	1,000–1,500 kg/h+
	National Cash Center / Banknote Printing Plant / Central Banks
	Solution A: Integrated Shredding & Briquetting
✔ (1/7) BM3002P-9075 – High-security integrated shredding & briquetting
✔ (2/7) BM6002P – Dual-stage shredding for high-capacity destruction
✔ (3/7) Models 5002 & 5001 – Shredding + baling combo



Case study • Client B
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📦 Recommended Models 
	Model 
	Type & Positioning 
	Target Scenario 
	Capacity / Throughput 
	Briquette / Baler
	Key Highlights 

	BM3002P-9075
	Integrated shredding + briquetting 
	Provincial / Municipal Destruction Room 
	100–150 kg/h @ 3 mm；~75 kg/h @ 1 mm
	Ø90×40 mm paper briquette 纸砖
	Closed feeding, dual-control, PLC HMI, video & weighing traceability 

	BM6002P
	Modular 1 mm mainline 
	Provincial Bank / Treasury Center 
	300–700 kg/h（scalable 
	Briquetter / Baler 
	Multi-point suction, long-run ducting, cross-room/floor 

	BM6002P (Parallel) + YKJ90-75 / 90-250
	High-throughput parallel line 
	National Cash Center / Banknote Printer 
	1000 kg/h+
	YKJ90-75 (single port) / YKJ90-250 (dual port)
	Scalable, low TCO, high uptime 

	BM4001
	Compact 1 mm upgrade 
	Small rooms / retrofit 
	250 kg/h+
	YKJ90-75 (single port) / YKJ90-250 (dual port)
	Quick fit-in; integrate with existing suction & briquetter 

	5002 (or 5001/500CC2024)
	Pre-shred + baling
	Pre-shred to offload main line
	500–600 kg/h（single line ）
	Bale 50–75 kg 
	Reduces main load & raises stability 

	YTJ-BM1 Series (300/400/500/600BM1)
	Ultra-fine 1×1 mm
	Classified room / Military / Finance
	80–500 pages per put
	—
	Belt-feed; handles thick bound files

	SL500 / SL600 / SL700
	Silent high-security
	Office / Voucher Room
	—
	—
	Low noise, compact footprint

	QL300–QL600
	Cost-effective line
	Small / Mid volume
	—
	—
	Budget-friendly；prefer bagging/boxing

	PSJ300 / 350 / 500 / 468
	Industrial pre-shred
	Books/archives pre-shred 
	100–1000+ kg/h
	—
	Dual-inlet, continuous duty 







🏛 Case Studies
· People’s Bank of China (PBOC) – Provincial Destruction Centers
· Shanghai Mint & Nanjing Mint – Banknote printing & recycling
· National Security Printing Plant – Integrated shredding + briquetting
· African & Asian Central Banks – YD-BM3002P customized destruction line
· Classified/confidential entity – YD-BM6002 ultra-fine (powder-grade) shredding system.

Case study • client C
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[bookmark: OLE_LINK11]Case study • client D
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Case study • client E 
A Central Bank in the Russian Region
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🌍 Compliance & Certification 
✔ DIN 66399 P-6 / P-7
✔ China National Level 1 Confidentiality Standard 

Why YUEDU 
· Aligned with international architectures (Standard / Modular / Tailored) covering the full process—feeding, shredding, suction, briquetting, and monitoring—while delivering lower cost and faster lead times.
· Integrated + modular approach: from small destruction rooms to national cash centers, with optional briquetting or bagging configurations.
✓ Proven technical capability in multi-stage shredding systems
✓ Compliance with central bank destruction standards
✓ Stable, durable, and safety-certified industrial machinery
✓ Experience integrating complete destruction lines
(coarse shredding → fine shredding → air conveying → dust removal → briquetting)
YUEDU is fully qualified to deliver:
· Safe
· Reliable
· International-standard
· Long-term maintainable
banknote destruction systems for the Central Bank. 
[bookmark: OLE_LINK4][bookmark: OLE_LINK5]
🌐 Contact Us 
Shanghai YUEDU Technology Co., Ltd.
🌐 Website: www.yuedushredders.com
📧 Email: yuedushredders@gmail.com / denghao8410@gmail.com
☎️  Sales Supervisor: +86 159 0178 2779  (WhatsApp / WeChat / Facebook / Telegram) 
📍 Company Headquarters: No. 555 Chengyin Road, Baoshan City Industrial Park, Shanghai, China
@YUEDUShredders – Empowering Global Industries with Intelligent Destruction Systems.
Specifications subject to change without prior notice.
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