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1. Project Overview
This solution is designed for professional document destruction operators providing outsourced services to banks and financial institutions.
The system focuses on long-term operational stability, security compliance, and cost efficiency, which are critical for service providers managing continuous workloads from multiple banking clients.
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· Total annual volume: approx. 2,000 tons
· Normal documents: 1,500 tons / year
· High-security documents (EU P6–P7): 500 tons / year
· Operational assumption:
· 200 working days per year
· 6 operating hours per day
· Site condition:
· Centralized operation at one facility
· Available area ≥ 500 m², height approx. 6 m
· Design objective:
· Stable, scalable operation for outsourced destruction services
· Clear separation of security levels for different banking requirements

2. Overall System Concept
The proposed system is designed specifically for operators, not for one-time or internal bank use.
· Normal and high-security documents are processed on separate, dedicated lines
· Parallel line architecture ensures:
· Continuous operation
· Easy maintenance without full shutdown
· Lower operational risk for service providers
· The system is suitable for multi-client, long-term service contracts

3. Line A – Normal Document Shredding (EU P2–P3)
Annual volume: approx. 1,500 tons
· Required throughput: 1.2–1.3 tons/hour
· Configuration: 2 parallel shredding lines
Each line includes:
· Primary shredder
· Motor power: 15 kW 
· Secondary shredder
· Motor power: 10 kW
· Security level: EU P2–P3
· Single-line capacity: 600–700 kg/hour
Discharge & baling:
· Shredded paper is sent directly to the customer’s existing baler
· Large paper bales for easy handling and resale
· No additional baler investment required

4. Line B – High-Security Document Shredding (EU P6–P7)
Annual volume: approx. 500 tons
· Required throughput: approx. 400–420 kg/hour
· Configuration: 2 parallel high-security shredding lines
Each line includes:
· Conveyor feeding system
· Primary shredder
· Motor power: 11 kW
· High-security fine shredder
· Motor power: 22 kW
· Output size: 1–2 mm particles
· Security level: EU P6–P7
· Single-line capacity: 150–200 kg/hour
Final treatment:
· Shredded paper powder is processed by a hydraulic briquetting system
· Compressed into small cylindrical briquettes

5. Key Advantages for Operators
· ✔ Designed for outsourced document destruction services
· ✔ Parallel production lines ensure high uptime and operational flexibility
· ✔ Separation of security levels improves workflow efficiency
· ✔ Industrial-grade design suitable for continuous daily operation
· ✔ Optimized investment structure and long-term ROI for operators 

This solution concept is intended for professional operators serving banks, central banks, and financial institutions. 

🌐 Contact Us 联系我们
Shanghai YUEDU Technology Co., Ltd. | 上海越都科技有限公司
📧 Email: yuedushredders@gmail.com | denghao8410@gmail.com 
📱 WhatsApp / WeChat: +86 159 0178 2779
🌐 Website: www.yuedushredders.com
@YUEDUShredders – Empowering Global Industries with Intelligent Destruction Systems.
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1. 项目概述（Project Overview）
本解决方案专为专业文件销毁运营方（Document Destruction Operators）设计，用于为银行及金融机构提供外包式档案销毁服务。
系统设计重点放在长期运行稳定性、保密合规性以及整体成本效率上，适用于需要同时服务多家银行客户、长期连续运行的运营场景。
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· 年总处理量：约 2,000 吨
· 普通文件：1,500 吨 / 年
· 高保密文件（EU P6–P7）：500 吨 / 年
· 运行假设：
· 每年 200 个工作日
· 每天 6 小时 实际运行时间
· 场地条件：
· 单一厂区集中运营
· 可用面积 ≥ 500 平方米
· 厂房高度约 6 米
· 设计目标：
· 适用于外包销毁服务的稳定、可扩展运营
· 不同保密资料对应不同保密等级，清晰分线处理

2. 整体系统设计理念（Overall System Concept）
该系统是从运营方视角出发设计的工业级方案，并非一次性项目或银行内部自用系统。
· 普通文件与高保密文件 分别在独立生产线上处理
· 并行生产线架构可实现：
· 连续稳定运行
· 单线维护时无需全线停机
· 降低运营方整体运行风险
· 系统非常适合：
· 多客户并行
· 长期服务合同
· 规模化档案销毁运营

3. Line A —— 普通文件粉碎线（EU P2–P3）
年处理量：约 1,500 吨
· 目标产能：约 1.2–1.3 吨 / 小时
· 配置方式：2 条并行粉碎生产线
每条生产线配置包括：
· 一级粉碎机（Primary Shredder）
· 电机功率：15 kW 
· 二级粉碎机（Secondary Shredder）
· 电机功率：10 kW 
· 保密等级：EU P2–P3
· 单线产能：约 600–700 kg / 小时
出料与打包方式：
· 粉碎后的纸张 直接进入客户现有打包机 
· 打包成大尺寸纸包，便于搬运、存储及再销售
· 无需额外投资新的打包设备

4. Line B —— 高保密文件粉碎线（EU P6–P7）
年处理量：约 500 吨
· 目标产能：约 400–420 kg / 小时
· 配置方式：2 条并行高保密粉碎生产线
每条生产线配置包括：
· 输送带自动上料系统
· 一级粉碎机
· 电机功率：11 kW
· 高保密细碎机
· 电机功率：22 kW
· 出料尺寸：1–2 mm 粉末颗粒
· [bookmark: OLE_LINK16]保密等级：EU P6–P7
· 单线产能：约 150–200 kg / 小时
末端收集和压块：
· [bookmark: OLE_LINK13][bookmark: OLE_LINK14]粉碎后的纸粉进入液压式纸粉压块系统
· 压缩成小型圆柱状压块

5. 运营方核心优势总结（Key Advantages for Operators）
· ✔ 专为外包式文件销毁运营模式设计
· ✔ 并行生产线保障高开机率与运营灵活性
· ✔ 不同保密等级分线处理，提升整体流程效率
· ✔ 工业级设计，适合长期、连续日常运行
· ✔ 投资结构合理，有利于运营方长期 ROI

本方案适用于为银行、中央银行及金融机构提供服务的专业运营方。 
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📞 Contact Us

Johnny Deng, Managing Director
☎️  Phone: +86 159 0178 2779 (WhatsApp / WeChat / Facebook / Telegram)
📧Email: denghao8410@gmail.com

Shanghai YUEDU Technology Co., Ltd. (YUEDU Shredders) 
🌐 Website(Global): www.yuedushredders.com (note: VPN required for China access, as the server is hosted by Google.)
📧 Email: yuedushredders@gmail.com / denghao8410@gmail.com
☎️  Sales Supervisor: +86 159 0178 2779  (WhatsApp / WeChat / Facebook / Telegram) ☎️  Administrative Supervisor: +86 137 6138 5116 
☎️  Head Office Main Line: +86 21 519 000 20
📍 Company Headquarters: Building 12, No. 555 Chengyin Road, Baoshan City Industrial Park, Shanghai, China



与我们联系（中文普通话）

上海越都科技有限公司
📍公司总部：上海市宝山城市工业园区城银路555弄12号楼
☎️  中文电话: 138 1115 0898（同微信）, 137 1700 3125（同微信）, 188 1682 6112（同微信）
☎️  公司总机：021 - 519 000 20
☎️  行政总裁：137 6138 5116
☎️  投诉电话：159 0178 2779
📧  Email邮箱: denghao8410@gmail.com
🌐 Website(中文网站): www.91suizhiji.com 
🌐 文档下载站： www.daxingsuizhiji.com 
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