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📄 Secure Document Destruction Solution – Normal & High-Security
Integrated Shredding Lines – 2,000 Tons / Year
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1. Project Overview
This project is designed for bank-related archival document destruction, combining operational efficiency and high security compliance.
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· Total volume: approx. 2,000 tons / year
· Normal documents: 1,500 tons / year
· High-security documents (P6–P7): 500 tons / year
· Operation assumption:
· 200 working days / year
· 6 operating hours / day
· Site condition:
· Single centralized location
· Area ≥ 500 m², height approx. 6 m
· Design objective:
· Stable, long-term industrial operation
· Modular & parallel production lines
· Clear separation of security levels

2. Overall System Concept
We recommend an integrated solution with separated security levels and parallel production lines:
· Normal documents and high-security documents are processed on independent lines
· Multiple parallel lines ensure:
· Operational stability
· Maintenance flexibility
· No single-point failure risk
· All systems are centrally managed within one facility

[bookmark: OLE_LINK11][bookmark: OLE_LINK8]3. Line A – Normal Document Shredding (EU P2–P3)
Annual volume: approx. 1,500 tons
· Required throughput: 1.2–1.3 tons/hour
· [bookmark: OLE_LINK10]Configuration: 2 parallel shredding lines
Each line includes:
· Primary shredder
· Motor power: 15 kW
· Output size: approx. 20 mm
· Secondary shredder
· Motor power: 10 kW
· Security level: EU P2–P3
· Single-line capacity: 600–700 kg/hour
Discharge & baling:
· Shredded paper is sent directly to the customer’s existing baler
· Large paper bales for easy handling and resale
· No additional baler investment required

[bookmark: OLE_LINK12]4. Line B – High-Security Document Shredding (EU P6–P7)
Annual volume: approx. 500 tons
· Required throughput: approx. 400–420 kg/hour
· Configuration: 2 parallel high-security shredding lines
Each line includes:
· Conveyor feeding system
· Primary shredder
· Motor power: 11 kW
· High-security fine shredder
· Motor power: 22 kW
· Output size: 1–3 mm particles
· Security level: EU P6–P7
· Single-line capacity: 150–200 kg/hour
Final treatment:
· Shredded paper powder is processed by a hydraulic briquetting system
· Compressed into small cylindrical briquettes
· Ensures maximum security and reduced volume

5. Key Advantages of the Integrated Solution
· ✔ Parallel line design for high reliability and redundancy
· ✔ Clear separation of normal and high-security workflows
· ✔ Industrial-grade operation, not an oversized single machine
· ✔ Suitable for long-term operation in banking and archival environments


🌐 Contact Us 联系我们
Shanghai YUEDU Technology Co., Ltd. | 上海越都科技有限公司
📧 Email: yuedushredders@gmail.com | denghao8410@gmail.com 
📱 WhatsApp / WeChat: +86 159 0178 2779
🌐 Website: www.yuedushredders.com
@YUEDUShredders – Empowering Global Industries with Intelligent Destruction Systems.

🏦 银行档案文件安全销毁整体解决方案 - 普通文件 + 高保密等级文件
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一、项目背景与目标
[bookmark: OLE_LINK9]本方案面向银行、金融机构及专业档案销毁运营方，
用于集中处理 普通文件 + 高保密等级文件（P6–P7） 的长期、安全、合规销毁需求。
核心目标：
· ✔ 满足不同保密等级的合规要求
· ✔ 连续稳定运行，适合长期外包运营

二、整体方案架构
本方案采用 “两套工艺 + 一个整体系统” 的设计理念：
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🔹 Line A｜普通文件粉碎 + 打包机
用于银行日常档案、普通文件集中处理
· 输送带自动进料
· 工业级粉碎机连续粉碎
· 粉碎后物料 直接进入打包机压块
· 压块成型，便于仓储与运输
👉 优势：
· 人工投入少
· 处理效率高
· 末端直接成块，降低物流成本

🔹 Line B｜高保密文件（EU P6–P7）粉碎成粉末 + 压块机
用于涉密文件、敏感档案、安全级别要求极高的文件
· 两条完全独立、结构相同的高保密粉碎线
· 每条线包含：
· 一级粗碎
· 二级细碎（达到EU P6–P7）,粉碎后为1~3mm粉末状
· 双线并行运行，保障连续性与冗余安全
· 粉碎后的纸粉进入液压式纸粉压块系统
· 压缩成小型圆柱状压块

[bookmark: OLE_LINK18][bookmark: OLE_LINK19]三、每年产能
· [bookmark: OLE_LINK20]年处理总量：约 2,000 吨 / 年
· 普通文件：约 1,500 吨/ 年
· 高保密文件：约 500 吨/ 年

四、适用客户类型
· 银行档案中心
· 金融机构集中销毁中心
· 第三方专业保密销毁运营商
· 政府或金融外包销毁项目

[bookmark: OLE_LINK17][bookmark: OLE_LINK39][bookmark: OLE_LINK40]

📞 Contact Us

Johnny Deng, Managing Director
☎️  Phone: +86 159 0178 2779 (WhatsApp / WeChat / Facebook / Telegram)
📧Email: denghao8410@gmail.com

Shanghai YUEDU Technology Co., Ltd. (YUEDU Shredders) 
🌐 Website(Global): www.yuedushredders.com (note: VPN required for China access, as the server is hosted by Google.)
📧 Email: yuedushredders@gmail.com / denghao8410@gmail.com
☎️  Sales Supervisor: +86 159 0178 2779  (WhatsApp / WeChat / Facebook / Telegram) ☎️  Administrative Supervisor: +86 137 6138 5116 
☎️  Head Office Main Line: +86 21 519 000 20
📍 Company Headquarters: Building 12, No. 555 Chengyin Road, Baoshan City Industrial Park, Shanghai, China



与我们联系（中文普通话）

上海越都科技有限公司
📍公司总部：上海市宝山城市工业园区城银路555弄12号楼
☎️  中文电话: 138 1115 0898（同微信）, 137 1700 3125（同微信）, 188 1682 6112（同微信）
☎️  公司总机：021 - 519 000 20
☎️  行政总裁：137 6138 5116
☎️  投诉电话：159 0178 2779
📧  Email邮箱: denghao8410@gmail.com
🌐 Website(中文网站): www.91suizhiji.com 
🌐 文档下载站： www.daxingsuizhiji.com 
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