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📄 Secure Document Destruction Solution - for Professional Operators
Integrated Shredding Lines - 2,000 Tons / Year
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1. Project Overview
This solution is designed for professional document destruction operators providing outsourced services to banks and financial institutions.
The system focuses on long-term operational stability, security compliance, and cost efficiency, which are critical for service providers managing continuous workloads from multiple banking clients.
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· Total annual volume: approx. 2,000 tons
· Normal documents: 1,500 tons / year
· High-security documents (EU P6–P7): 500 tons / year
· Operational assumption:
· 200 working days per year
· 6 operating hours per day
· Site condition:
· Centralized operation at one facility
· Available area ≥ 500 m², height approx. 6 m
· Design objective:
· Stable, scalable operation for outsourced destruction services
· Clear separation of security levels for different banking requirements

2. Overall System Concept
The proposed system is designed specifically for operators, not for one-time or internal bank use.
· Normal and high-security documents are processed on separate, dedicated lines
· Parallel line architecture ensures:
· Continuous operation
· Easy maintenance without full shutdown
· Lower operational risk for service providers
· The system is suitable for multi-client, long-term service contracts

3. Line A – Normal Document Shredding (EU P2–P3)
Annual volume: approx. 1,500 tons
· Required throughput: 1.2–1.3 tons/hour
· Configuration: 2 parallel shredding lines
Each line includes:
· Primary shredder
· Motor power: 15 kW 
· Secondary shredder
· Motor power: 10 kW
· Security level: EU P2–P3
· Single-line capacity: 600–700 kg/hour
Discharge & baling:
· Shredded paper is sent directly to the customer’s existing baler
· Large paper bales for easy handling and resale
· No additional baler investment required

4. Line B – High-Security Document Shredding (EU P6–P7)
Annual volume: approx. 500 tons
· Required throughput: approx. 400–420 kg/hour
· Configuration: 2 parallel high-security shredding lines
Each line includes:
· Conveyor feeding system
· Primary shredder
· Motor power: 11 kW
· High-security fine shredder
· Motor power: 22 kW
· Output size: 1–2 mm particles
· Security level: EU P6–P7
· Single-line capacity: 150–200 kg/hour
Final treatment:
· Shredded paper powder is processed by a hydraulic briquetting system
· Compressed into small cylindrical briquettes

5. Key Advantages for Operators
· ✔ Designed for outsourced document destruction services
· ✔ Parallel production lines ensure high uptime and operational flexibility
· ✔ Separation of security levels improves workflow efficiency
· ✔ Industrial-grade design suitable for continuous daily operation
· ✔ Optimized investment structure and long-term ROI for operators 

This solution concept is intended for professional operators serving banks, central banks, and financial institutions. 

🌐 Contact Us 联系我们
Shanghai YUEDU Technology Co., Ltd. | 上海越都科技有限公司
📧 Email: yuedushredders@gmail.com | denghao8410@gmail.com 
📱 WhatsApp / WeChat: +86 159 0178 2779
🌐 Website: www.yuedushredders.com
@YUEDUShredders – Empowering Global Industries with Intelligent Destruction Systems.
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📞 Contact Us

Johnny Deng, Managing Director
☎️  Phone: +86 159 0178 2779 (WhatsApp / WeChat / Facebook / Telegram)
📧Email: denghao8410@gmail.com

Shanghai YUEDU Technology Co., Ltd. (YUEDU Shredders) 
🌐 Website(Global): www.yuedushredders.com (note: VPN required for China access, as the server is hosted by Google.)
📧 Email: yuedushredders@gmail.com / denghao8410@gmail.com
☎️  Sales Supervisor: +86 159 0178 2779  (WhatsApp / WeChat / Facebook / Telegram) ☎️  Administrative Supervisor: +86 137 6138 5116 
☎️  Head Office Main Line: +86 21 519 000 20
📍 Company Headquarters: Building 12, No. 555 Chengyin Road, Baoshan City Industrial Park, Shanghai, China
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