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Looking for complete solutions for banknote destruction? 
This comprehensive video covers 3 major strategies and 7 specialized models trusted by central banks:

Solution A: Integrated Shredding & Briquetting
✔ (1/7) BM3002P-9075 – High-security integrated shredding & briquetting 
✔ (2/7) BM6002P – Dual-stage shredding for high-capacity destruction 
✔ (3/7) Models 5002 & 5001 – Shredding + baling combo
Solution B: Ultra-Fine 1mm Shredding System
✔ (4/7) 300BM1 – 600BM1 Series – Ultra-fine shredding (1mm) for P-6 compliance 
✔ (5/7) Modular Systems 6002 & 4001 – Customizable with briquetting/baling
Solution C: Cost-Effective 1–3mm Shredding
✔ (6/7) QL300 – QL600 Series – Budget-friendly shredders from $2,000 
✔ (7/7) SL500 – SL700 Series – Silent, high-security shredding for offices
👉 Learn more: www.yuedushredders.com
[bookmark: OLE_LINK3]

📄 （1/7）BM3002P-9075 Banknote Shredding & Briquetting System
Paper Shredder with Integrated Baler and Compactor
YUEDU Brand | Model: BM3002P-9075
	Banknote Destruction Machine
	Integrated Baler and Compactor
	Output
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Shredder Specifications
	•	Single Feed Capacity: 100 sheets; Hourly Shredding Capacity: 100-150KG/H
	•	Feed Width: 420mm    •	Power: 22KW 
	•	Dimensions: 3380*1440*2220mm
Shredding Process:
	•	Two-stage shredding with dual blade sets.•	Dimensions: 1480*1440*1850mm
	•	Output: 3mm particles: 100-150KG/H; 1mm particles: 75KG/H
Compacting Process:
	•	Compressed block diameter: 90mm*40mm; Compacting output: 75KG/H
	•	Dimensions: 1900*1400*2220mm

	User Case: Banknote Shredder and Compactor Combo Machine

	Overall Image
	Compactor Section
	Output 
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	https://youtu.be/OnOKqf-vkCA 

https://youtube.com/shorts/5-dmXbM1Wpw 
	https://b23.tv/Go7TGFH 

https://b23.tv/ToFqYLg 


[bookmark: _Toc198829082]📄（2/7）YD-BM6002P Integrated Shredding System 
All-in-One Shredding, Dust Collection & Baling System
Integrated system solutions for shredding, secondary processing, dust removal, and baling.
🖼️ Product Overview 
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🧩  Application Scenarios
🔒🛡️Secure / Confidential Room
🔒🏭 Secure Destruction Center
💰 Product Pricing:
Shredder Unit – Model: YD-BM6002 → ¥497,731
Baler & Compactor Unit – Model: YD-DBJ6002P → ¥497,500
📏 System Overview: Three-View Diagram
(Front / Side / Top Views of the Integrated System)
[image: ]
📌 Note:The above solution is for reference only. Final delivery is subject to the user’s confirmed requirements.
[bookmark: _Toc198829028][bookmark: _Toc198829030]
📄（3.1/7） YD-500CC2024 (500 pages)
🖼️ Product Overview
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🔧 Technical Specifications： 
	🔒Security Level (DIN 66399)
	P-2/O-2/T-2/E-2
	P-3/O-2/T-3/E-2
	P-4/O-3/T4/E-3
	P-5/O-4/T5/E-4/F-2

	📥Feed Width (mm)
	500
	500
	500
	500

	✂️ Cut Size(mm)
	10.5x40-75
	6x50
	3.8x40
	1.9x15

	📑 Max Sheets
	500-550
	340-380
	180-200
	90-100

	⚖️Weight (kg)
	1200
	1200
	1200
	1200

	🔌Power
	7.5KW
3 x 400 V/50 Hz
	7.5KW
3 x 400 V/50 Hz
	7.5KW
3 x 400 V/50 Hz
	9.5KW
3 x 400 V/50 Hz

	📏 L×W×H (mm)
	1318×1843×1638
	1318×1843×1638
	1318×1843×1638
	1318×1843×1638

	🗑️Bin(L)
	550L
	550L
	550L
	550L

	💰Price (USD)
	
	
	
	


➕ Optional Add-ons:
Floor-mounted conveyor and rear baling system for efficient shredding and compact waste handling.

📄（3.2/7）YD-5002 Book Shredding & Baling Systems
🖼️ Product Overview
[image: ] [image: ]
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500CC shredder + 10T baler combo, ideal for secure rooms and archives. 
Shreds up to 500 kg/h, compresses into 50–75 kg paper bales. 
🔧 Technical Specifications：  
⚙️Output/h: 500–600 kg
⚖️ Bale Weight: 50–75 kg
🧱Baling Pressure: 85 kN
🔌Power: 11.5 kW, 3 phase 400 V / 50 HZ
📏 L×W×H (mm): 3257*2588*2284
📐 System Overview: Three-View Diagram
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[bookmark: _Toc198829077]
[bookmark: _Toc198829078]📄（4/7）YD-YTJ600BM1 500 400 300 – 1mm Ultra-Fine Shredders
🖼️ Product Overview
	📸On-Site Usage
	[image: ]  

	🌫️Shredding Result
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✂️ Shreddable Materials
Books and paper documents, CDs/DVDs
Cards and chip-based items (e.g. SIM cards, mobile chips)
PVC advertising boards, plastic display panels, KT boards, school and institutional event panels
Other paper- or fiber-based media
Other plastic-based materials
🔧 Technical Specifications
	🆔Model
	YD-YTJ600BM1
	YD-YTJ500BM1
	YD-YTJ400BM1
	YD-YTJ300BM1

	📥Feed Width
	60CM*38CM
	50CM*30CM
	40CM*26CM
	30CM*22CM

	✂️ Cut Size
	1*1mm粉末状，可调整粉碎尺寸为1*2mm, 8mm, 3mm等

	📑 Max Sheets
	300-500
	200-300
	100-200
	80-130

	🔌Power
	19.12KW,3 phase 380V
	15KW,3 phase 380V
	10KW,3 phase 380V
	7.5KW, 3 phase 380V

	💰Price (USD)
	29,610
	21,150
	21,150
	17,143


➕ Custom Case
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[bookmark: _Toc198829080][bookmark: _Toc198829079]📄（5.1/7）YD-BM6002– Modular 1mm Shredding Solutions
Flagship 1mm Powder-Level Security Shredding System
🖼️ Product Overview
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🧩 Application Scenarios
[bookmark: OLE_LINK90]🔒🛡️ Secure / Confidential Room / Secure Destruction Center

💰 Price: RMB 497,731

🔧 Technical Specifications
	Model
	YD-BM6002
	📏整体方案三视图：

	[bookmark: _Hlk217044319]Feed Opening Size
	600 mm (W) × 280 mm (H)
	[image: ]

	[bookmark: OLE_LINK92]Shredding Output Form
	Powder (adjustable)
	

	Minimum Particle Size
	1 × 1 mm
	

	Shredding Capacity
	1×2 mm: 80–100 kg/hour
4–5 mm: 500–650 kg/hour
8 mm: 1200–1600 kg/hour
	

	Sheets per Batch
	300–500 sheets
	

	Power Supply
	380 V / 3-phase
	

	Installed Power
	27 kW
	



➕ Case
	[bookmark: OLE_LINK98][bookmark: OLE_LINK99][image: ]
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📌 Note:The above solution is for reference only. Final delivery is subject to the user’s confirmed requirements.

📄（5.2/7）YD-BM4001 – Modular 1mm Shredding Solutions
[image: ][image: ]
	1mm powder - 1mm粉末状
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Shredder Specifications:
	•	Single Feed Capacity: 100 sheets; Hourly Shredding Capacity: 100-150KG/H
	•	Output: 3mm particles: 100-150KG/H; 1mm particles: 75KG/H
[image: ]  https://www.youtube.com/watch?v=Kc4YdBsiQKo 
➕ Custom Case定制案例
	Banknote Destruction Machine
	Integrated Baler and Compactor
	Output
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[bookmark: _Toc198829040][image: ]  Video1: https://youtu.be/OnOKqf-vkCA     Video2: https://youtube.com/shorts/5-dmXbM1Wpw 
📄（6/7）YD-FSJQL系列 300-800型漏斗大功率机型
🖼️ Product Overview
	YD-FSJQL300
	YD-FSJQL400
	YD-FSJQL500
	YD-FSJQL600
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Constructed with specialized wear-resistant steel, this innovative design guarantees unmatched bite force, exceptional durability, and an extended service life. The oversized inertia wheel amplifies torque and maximizes capacity, ensuring peak performance under demanding conditions.

Technical Specifications:
	Product Model
	YD-FSJQL300
	YD-FSJQL400
	YD-FSJQL500
	YD-FSJQL600
	YD-FSJQL800

	Inlet Dimensions (mm)
	310*260
	410*260
	510*260
	610*310
	810*410

	Number of Sheets Shredded[footnoteRef:1] [1:  For Long-Term Operation: Feed materials evenly and wait until the materials in the shredding chamber are fully processed before adding more. For continuous feeding, ensure each batch is no more than one-third of the value specified in the table.] 

	30-50
	70-80
	100-150
	200-300
	400-800

	Shredding Capacity[footnoteRef:2]（kg/h） [2:  Shredding Capacity: The listed capacity is the maximum, applicable to hard plastics. For materials like paper, the shredding capacity decreases and depends on the output size (larger sizes process faster). For shredding paper, a 3 cm output size is recommended for faster processing.] 

	100-200
	150-250
	200-350
	300-600
	500-800

	Motor Power
	5.5KW, 380V
	7.5KW, 380V
	11KW, 380V
	15KW, 380V
	30KW, 380V

	Shredded Size(Customizable) [footnoteRef:3] [3:  Customizable Sizes: Available in 1mm, 3mm, and 5mm specifications. For additional options, please contact customer service.] 

	8mm 
	8mm 
	8mm 
	8mm 
	8mm 

	Dimensions (m)
	1.22x0.72x1.16
	1.32x0.86x1.46
	1.45x1.00x1.54
	1.70x1.15x1.88
	2.22x1.38x2.38

	Weight (kg)
	450
	550
	750
	850
	2000

	Pricing RMB
	11765
	15261
	19792
	31423
	79618


[bookmark: _Toc198829046]📄（7/7）YD-SL500 | 600 | 700 Silent High-Power Shredder
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	[bookmark: _Hlk186201993]Front View
	Internal View
	Safe Feeding Inlet
	Fully Enclosed Waste Bin


🏆Twenty Years of Design Expertise, Proven Client Applications, and Innovative Global Technologies
As a pioneering new product, it integrates two decades of engineering excellence, extensive client application cases, and globally innovative technology. Features include but are not limited to:
	● EHS-Compliant: Fully aligned with global Environmental, Health, and Safety standards, trusted by multinational corporations.
● High Efficiency, Low Energy Consumption: Saves costs while delivering exceptional performance.
● Zero Leakage: No material leakage, no dust emissions, and no material return during operation.
	● Handles Extreme Materials: Suitable for ultra-thick and super-hard materials.
● Adaptable to Low-Melting Plastics and Rubber: Ideal for processing heat-sensitive materials.
● Compatible with Glass Fiber and Mineral Materials: Designed for tough, abrasive substances.


🌍Preferred by Industry Leaders
The first choice for multinational corporations, industry leaders, and Fortune Global 500 enterprises.
🔧Technical Specifications:
	[bookmark: _Hlk177551093]Product Model
	YD-SL500
	YD-SL600
	YD-SL700
	YD-SL800

	Inlet Dimensions (mm)
	400*250
	500*260
	600*300
	700*500

	Number of Sheets Shredded[footnoteRef:4] [4:  For Long-Term Operation: Feed materials evenly and wait until the materials in the shredding chamber are fully processed before adding more. For continuous feeding, ensure each batch is no more than one-third of the value specified in the table.] 

	150-250
	300-500
	400-600
	500-700

	Shredding Capacity[footnoteRef:5] [5:  Shredding Capacity: The listed capacity is the maximum, applicable to hard plastics. For materials like paper, the shredding capacity decreases and depends on the output size (larger sizes process faster). For shredding paper, a 3 cm output size is recommended for faster processing.] 

	200-350 kg/h
	300-600 kg/h
	400-600kg/h
	500-700kg/h

	Motor Power
	7.5KW, 380V
	11KW, 380V
	15kw, 380V
	30kw

	Shredded Size(Customizable) [footnoteRef:6] [6:  Customizable Sizes: Available in 1mm, 3mm, and 5mm specifications. For additional options, please contact customer service.] 

	8mm
	8mm 
	8mm
	8mm

	Dimensions (mm)
	840*1000*1563
	994*1160*1689
	1260*1200*1950
	1300*1250*2400

	Weight (kg)
	450
	700
	900
	1200

	Pricing RMB
	67669
	82715
	97761
	119837

	Pricing USD
	9,667
	11,817
	13,966
	17,120



📄 YD-FSJQL800 Industrial High-Performance Strong Cutter Shredder
[bookmark: OLE_LINK260]🖼️ High-performance shredding unit for heavy-duty, multi-material applications. 
[image: ]
[image: ][image: ][image: ] It is capable of processing bulk paper but also excels at shredding large, thick, and hard engineering plastics and other diverse materials.
[bookmark: OLE_LINK259]Its unique modular design allows it to operate as a high-efficiency standalone unit or integrate seamlessly into large-scale automated destruction or recycling production lines.
🌟 Key Advantages
· Powerful Shredding Performance / Integrated Conveying Structure 
· Flexible Modular Design / Industrial-Grade Throughput
🔧 Technical Specifications
	Model
	YD-FSJQL800

	Feed Opening
	810 * 410 mm (Ideal for bulk/boxed feeding)

	Motor Power
	30 KW, 380 V (High-torque drive)

	Throughput
	500 - 800 kg/h

	Max Sheets
	400 - 800 sheets (For paper-based materials)

	Discharge Structure
	Integrated Fan (Easy connection to suction systems)

	Output Size
	8 mm (Customizable upon request)

	Dimensions
	2.22 x 1.38 x 2.38 m





[bookmark: OLE_LINK150][bookmark: OLE_LINK151][bookmark: OLE_LINK152]📄 Ultra-High Security - Selection 9
Equivalent to DIN 66399 P-7 | 1×1 mm Powder Output– v12
	[bookmark: _Hlk103937822]

	Plan 1:
YD-YTJ400BM1
YD-YTJ500BM1
YD-YTJ600BM1
	Plan 2:
YD-BM4001
	Plan 3：
YD-BM4002
	Plan 4：
YD-BM6001

	Plan 5：
YD-BM6002
	Plan 6：
YD-BM6002P
	Plan 7：
YD-BM9002
YD-BM9002P

	Pricing USD
	300BM1, 17,143
400BM1, 21,150
500BM1, 25,380
600BM1, 29,610
	21,150
	63,450
	54,990
	70,500
	141,000
	9002, 141,000
9002P, 282,000

	Entry Image
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	Full Machine Image
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	Crushing efficiency
	35 / 40 / 45KG/H

	100KG/H
	60KG/H
	50KG/H
	80KG/H
	80KG/H
	150KG/H

	Shredded Size
	1*1mm
Adjustable, e.g. 2/5mm etc.
	1*1mm
	1*1mm
	1*1mm
	1*1mm
	1*1mm
	1*1mm

	Sheets Shredded
	100-300 sheets
	300-500 sheets
	200-300 sheets
	300-500 sheets
	300-500 sheets
	300-500 sheets
	300-500 sheets

	Entry Size
	40/ 50 / 60 CM
	60CM
	40CM
	60CM
	60CM
	60CM
	90CM

	Applicable Scenarios
	County-level units
	Provincial and municipal units
	Provincial and municipal
	County-level
	Provincial and municipal units
	Provincial/Headquarters
	Organizational Headquarters

	[image: ]
	https://youtu.be/q9D_uf_TdZI 
	https://youtu.be/RU7OpMIkUoc 
	https://youtube.com/shorts/KMaiAuUlj0s 
	https://youtu.be/i_cCRB-VJRw 
	https://youtu.be/v419WXU13oc 
	https://youtube.com/shorts/p3rOTUcy4Zg 
	https://youtube.com/shorts/p3rOTUcy4Zg 


 Attachment: Sample Display | 附件：样品展示
	1mm powder - 1mm粉末状
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	Compressed paper powder block - 纸粉压块
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	Compressed Money (RMB) block - 金钱（人民币）压块
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📞 Contact Us

Johnny Deng, Managing Director
☎️  Phone: +86 159 0178 2779 (WhatsApp / WeChat / Facebook / Telegram)
📧Email: denghao8410@gmail.com

Shanghai YUEDU Technology Co., Ltd. (YUEDU Shredders) 
🌐 Website(Global): www.yuedushredders.com (note: VPN required for China access, as the server is hosted by Google.)
📧 Email: yuedushredders@gmail.com / denghao8410@gmail.com
☎️  Sales Supervisor: +86 159 0178 2779  (WhatsApp / WeChat / Facebook / Telegram) ☎️  Administrative Supervisor: +86 137 6138 5116 
☎️  Head Office Main Line: +86 21 519 000 20
📍 Company Headquarters: Building 12, No. 555 Chengyin Road, Baoshan City Industrial Park, Shanghai, China



与我们联系（中文普通话）

上海越都科技有限公司
📍公司总部：上海市宝山城市工业园区城银路555弄12号楼
☎️  中文电话: 138 1115 0898（同微信）, 137 1700 3125（同微信）, 188 1682 6112（同微信）
☎️  公司总机：021 - 519 000 20
☎️  行政总裁：137 6138 5116
☎️  投诉电话：159 0178 2779
📧  Email邮箱: denghao8410@gmail.com
🌐 Website(中文网站): www.91suizhiji.com 
🌐 文档下载站： www.daxingsuizhiji.com 
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Attachment: Sample Display | Bii#F: H2R7
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